**Trouble Shooting**

**No Power**

1. Check position of on/off switch, the switch should be in the “up” or “on” position.
2. Check battery has adequate charge to power the machine. Must have at least 12 volts on meter.
3. Examine connections to the battery and the on/off switch. All connections should be secure.

**No water pumping (but pump is running).**

1. Remove quick disconnect to examine suction tube to the tank for any obstructions.
2. Check water level in tank; water must cover the intake to the suction tube.
3. Open a drinking valve and allow pump to prime and deliver water to the valve. Pump will turn off when valve is released.

**Water spraying when machine is turned on.**

1. Examine for valves that are bent to the side, close valves.
2. Remove air from the lines when starting the machine. Machine will sputter and spray water until all nozzles are pressurized and closed.

**Team Mate**

Assembly & Operating Instructions



 ***Wizard Sports
 877-559-5425***

**Dolly Assembly**

1. Place large washer over dolly axle.
2. Slide wheel onto dolly axle with the protruding center piece towards the dolly.
3. Place large washer, then use small washer if there is play at the cotter pin.
4. Insert cotter pin through hole in axle and slightly bend pin.
5. Repeat process for both wheels.

Sa

Sa

Axle Bracket

Cotter Pin

 Wheel

Wheel

 axle

Axle Bracket Small Washers

Large Washer Cotter pin

a

Small Washer (if needed)

Large Washers Cotter Pin

 **Safety Concerns**

1. When moving the Team Mate while full, it is important to control dolly at all times.
2. To avoid injury, when moving uphill, it is essential the user pull the dolly up a hill. DO NOT attempt to push a dolly up a hill. When moving the Team Mate down a hill, allow the dolly to roll down the hill with the operator in the uphill position. To ensure safety, do not roll downhill when objects or people are in front of the machine.

**Operating Instructions**

1. Charge battery overnight. Plug cord end of charger into the charging port located at the bottom of pump enclosure. Plug charger electrical prongs into 110V standard wall outlet. The light on the charger will turn from red to green when battery is fully charged. A full charge can take up to 12 hours (overnight).
2. Plug suction tube into quick disconnect at rear of tank.
3. Fill container with water or drinking fluids and ice. Secure top.
4. Push switch to “on” position. Voltage meter should show at least 12 volts for proper operation. 13.2v is optimal.
5. Open one drinking valve by bending the tip to the side with your thumb. Once steady stream of liquid is flowing, release drinking valve. Pump will automatically shut off. Purge air from other 5 valves in a similar matter.
6. Roll Team Mate utilizing Safety Concerns stated to desired location.
7. When finished, release the pump suction tube from the quick disconnect on bottom of tank. During transport, the Team Mate will drain itself.
8. Wipe the inside of the container with a clean/dry towel. Leave container open to allow any remaining moisture to evaporate. This reduces the chance of mold, fungus, or bacterial growth.
9. Occasionally inspect hoses for mold growth. If apparent, replace hose.

**Cleaning**

1. If fluids other than water are used, thoroughly rinse plumbing system with fresh water for 2 minutes.
2. A 10% bleach solution may be used for cleaning and storage.